[image: A close-up of a logo

Description automatically generated]STORMWATER DRAINAGE CONNECTIONS 

CITY OF VINCENT POLICY MANUAL TECHNICAL SERVICES - ENGINEERING, ASSET AND DESIGN SERVICES POLICY NO:  2.2.10
STORMWATER DRAINAGE CONNECTIONS



POLICY NO: 2.2.10



STORMWATER DRAINAGE CONNECTIONS 


	

Legislation / local law requirements
	
Metropolitan Arterial Drainage Act 1982

Metropolitan Water Supply, Sewerage and Drainage Act 1909

Waterways Conservation Act 1976

	
Relevant delegations
	
2.2.3 Performing particular things on land which is not Local Government Property.

	Related policies, procedures and supporting documentation
	Local Government Decision Making Hierarchy - D20/148390
Policy Registers - D20/126085 and Review Plan - D21/3270
State Planning Framework Planning Guidelines - Local Government Guidelines for Subdivisional Development





STORMWATER DRAINAGE CONNECTIONS

OBJECTIVES

the controlled disposal of stormwater from commercial, and residential properties.

INTRODUCTION
[bookmark: _Hlk164870517]The sustainable management of stormwater discharge is essential to all urbanised environments. Local Governments are responsible for controlling disposal of stormwater from commercial, industrial, and residential properties.
PURPOSE
[bookmark: _Hlk164870557]The purpose of this policy is to ensure that stormwater generated from commercial, industrial, and residential property within the City of Vincent is managed in a sustainable manner with particular regard to preserving the capacity of the City’s stormwater drainage infrastructure.
OBJECTIVE
[bookmark: _Hlk164870583]To specify the management requirements for the disposal of stormwater on commercial, industrial, and residential property within the City of Vincent.
SCOPE
[bookmark: _Hlk164870635]Commercial, industrial, and residential property in the City of Vincent and the City’s stormwater drainage infrastructure.
DEFINITIONS
Average recurrence interval (ARI)
The long-term average number of years between the occurrence of a flood as big as, or larger than, the selected event. For example, floods with a discharge as great as, or greater than, the 20-year ARI flood event will occur on average once every 20 years. ARI is another way of expressing the likelihood of occurrence of a flood event.

Retention System
Process or a design that involves keeping a portion of something (stormwater) for a certain purpose (avoid flooding).

Stormwater
Surface water in abnormal quantity resulting from heavy falls of rain.


POLICY STATEMENT

Disposal of stormwater generated on the following categories of property shall be as indicated:

Note:  to be read in conjunction with Planning Policy No. 3.5.9.

1.        Commercial or Developments

For properties where the nature of the soil is such that soakage is limited or not possible (as verified by a Geotechnical Report), an on-site stormwater water retention system capable of accommodating a minimum 1:10 year storm event is required from which a controlled overflow to the City’s drainage system may be permitted..

The cost of connecting to the City’s drainage system shall be borne by the
applicant.

If, however, the City does not have drainage infrastructure adjacent the property, or where the existing system is not capable of handling the additional flow,  the  stormwater  must  either  be  fully  compensated  on  site  or  an application made by the owner of the property to either extend or upgrade the stormwater system.   Where there is concern about possible pollution of the stormwater generated on such a property, the stormwater should be adequately treated and retained on site or other approved disposal methods applied.

2.        Residential

All stormwater is to be retained on-site.   If, however, circumstances exist where stormwater cannot be suitably retained  on-site, a connection to the City’s drainage system may be approved, subject to adequate compensation equivalent to a minimum 1:5 year storm event, being provided on the site.

The cost of connecting on-site drainage to the City’s drainage system shall be the responsibility of the owner of the property being connected and this includes the cost of any necessary extensions to the City’s drainage system.
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 POLICY

1. All stormwater generated from commercial, industrial, and residential property is to be retained on-site.
1. An on-site retention system is to meet the following capacity requirement – 

1. Commercial and Industrial Property
An on-site retention system capable of accommodating a minimum 1:100-year average recurrence interval (ARI) storm event of one hour is required.

1. Residential Property
An on-site retention system capable of accommodating a minimum 1:20-year average recurrence interval (ARI) storm event of one hour is required.

1. Technical design for on-site retention systems shall adhere to the drainage management requirements specified in the State Planning Framework Planning Guidelines - Local Government Guidelines for Subdivisional Development.
1. Connection to the City’s stormwater drainage infrastructure may be approved only in exceptional circumstances where stormwater runoff cannot be suitably retained on-site. 
1. Approval to connect to the City’s stormwater drainage infrastructure will be subject to the maximum on-site retention being provided according to prevailing site conditions. 
1. The cost for connection to, and any necessary upgrade of the City’s existing stormwater drainage infrastructure shall be borne by the applicant. 
1. Connections to the City’s stormwater drainage infrastructure shall consist of a controlled overflow into the system and upgrades will be sustainability focused and factor in future climate change considerations. 
1. Connections to the City’s stormwater drainage infrastructure shall be constructed and maintained in accordance with the specifications and conditions of approval determined by the City.
1. Stormwater discharged into the City’s stormwater drainage infrastructure is to be pollutant free. Where there is a risk of pollution of the stormwater generated from the property, the stormwater should be adequately treated and retained on site or other approved disposal methods applied.
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